SECTION 09 78 13

Alumiline Linear Metal Wall Planks with Reveal

**PART 1 GENERAL**

1. **SECTION INCLUDES**
   1. Extruded aluminum linear wall planks with reveal.
   2. Accessories for wall installation.
2. **SUBMITTALS**
   1. Product Data: Manufacturer’s technical data sheet and installation instructions for each type of wall plank required.
   2. Shop Drawings: Submit shop drawings, including details, for all walls. Coordinate wall layout, installation, and components with construction elements that penetrate walls or are supported by them. Show overall layout with dimensions and details for penetrations and intersections with other materials or building components.
   3. Samples: Submit three (3) full size samples of each plank type required.
   4. Certificates: Submit manufacturer’s certificate that products meet or exceed specified requirements.
   5. Test Reports: Upon request, submit certified test reports from recognized test laboratories.
3. **MAINTENANCE MATERIAL**
4. Extra Materials:
   * 1. Deliver no less than two percent (2%) of each type, color and pattern of material.
     2. Extra materials shall be from the same production run as the original materials.
     3. Extra materials shall remain in the manufacturer’s original packaging and given to the building owner upon substantial completion of the work. Store extra materials per instructions as described in storage and handling requirements.
5. **QUALITY ASSURANCE**
   1. Qualifications:
      1. Manufacturers: Provide linear metal wall planks with reveal from a single manufacturer.
      2. Installers: Utilize an installer having demonstrated experience on projects of comparable size and complexity.
6. **DELIVERY, STORAGE, AND HANDLING**
   1. Storage and Handling Requirements:
      1. Deliver material in the manufacturer’s original, unopened, undamaged containers with identification labels intact.
      2. Handle products carefully to avoid damage.
      3. Store materials protected from exposure to harmful environmental conditions and at temperature and humidity conditions recommended by the manufacturer.
7. **SITE CONDITIONS**
   1. Ambient Conditions:
      1. Maintain ambient temperature and humidity conditions at levels indicated for the project when occupied for its intended use.
      2. Do not install products under environmental conditions outside manufacturer’s recommended limits.
   2. Existing Conditions: Do not install linear metal wall planks until space is enclosed and weather proofed, wet work is completely dry, and work on walls is complete.
8. **WARRANTY**
   1. Provide manufacturer’s written product warranty per Section 01 77 00 – Closeout Procedures.

**PART 2 PRODUCTS**

1. **MANUFACTURERS**
   1. ASI Architectural, 123 Columbia Court N, Chaska, MN 55318.  
      Phone: 888-258-4637. Fax: 952-448-2613. Website: www.asiarchitectural.com
2. **DESCRIPTION**
   1. Product Description: Alumiline linear metal wall planks with reveal as manufactured by ASI Architectural.
   2. Product Options: For each item listed below, please select one (1) option from the choices.
      1. Construction: (Extruded aluminum linear plank sections)
      2. Finish: (Anodized) / (Powder Coat)
      3. Finish Color: (To match architect sample) / (Custom)
      4. Plank Width: (3-1/4") / (5-1/4")
      5. Reveal Width: (3/4”)
      6. Length: (10’) / (Custom)
3. **ACCESSORIES**
4. Attachment hardware for wall planks as specified by manufacturer for installation.
5. Spline for alignment.
6. Class A FR MDF blocking.
7. Accessories with Options: Select one (1) option from the choices for of the following accessories.
   1. (Felt - Interior) / (ABS – Exterior) Filler strip.
   2. Acoustical backer: (1") / (2") x 24" x 48". Black.
   3. F-channel vertical trim: 3/4" x (4") / (Custom) x (120"). F-channel vertical trim finish to match finish of wall planks.

**PART 3 EXECUTION**

1. **EXAMINATION**
   1. Verification of Conditions:
      1. Inspect installation area and conditions under which work is to be performed for compliance with all manufacturers’ environmental requirements.
      2. All wet work in the installation area must be complete, cured, and dry prior to installation.
      3. Wall assembly shall be complete, inspected, and accepted before wall work begins.
2. **INSTALLATION**
3. Comply with manufacturer’s instructions and recommendations for installation of wall planks and industry standards.
4. Coordinate the exact size, location, and sequencing of penetrations of wall planks by all building components.
5. Lay out wall pattern per approved shop drawings if required. Where not otherwise indicated, lay out planks so margins on opposite sides of rooms are equal or greater than half (1/2) the plank width.
6. **ADJUSTING**
7. Adjust planks after installation so that surfaces are aligned, flush, and level with gaps between units consistent in width and straight.
8. **CLEANING**
9. Clean surfaces of wall planks per manufacturer’s instructions.
10. Remove and replace damaged or discolored material and material that cannot be properly cleaned.
11. **PROTECTION**
12. Protect installed work from damage due to subsequent construction activity, including temperature and humidity limitations and dust control, so that the work will be without damage and deterioration at the time of acceptance by the owner.

END OF SECTION